$Topology Optimization Input File
FeederSystem1=Static,Static22,22,D:\ANSYS_EX\C11\LShape_files\dp0\SYS\MECH\,1,1.000000
nonlin_contact = no
min_density = 0.001
power_law_stiff = 3
max_iter = 500
acc = 0.001
output_freq = 1
max_num_inter_files = 500
solver = scpip
ansys_version = 195
units = MPA
distributed = True
num_procs = 2

cut_off_scp = 1
version_scp = 402

$Objective:
objective1=COMP,Objective,22,all,no,1

$Constraints:
constraint1 = TOT_MASS,Mass Constraint, 25

$Design Space:
design_elements = OptimizationRegionElements.dat

$Capability Info:
license_server = 50137@127.0.0.1
capability_id = E109-Works-E109-12468-012405
